Harness status: OK

Found 88 tests

88 Pass
Pass	cSHAKE128 with 0 bit output and empty source data
Pass	cSHAKE128 with 0 bit output and short source data
Pass	cSHAKE128 with 0 bit output and short source data and altered buffer during call
Pass	cSHAKE128 with 0 bit output and short source data and altered buffer after call
Pass	cSHAKE128 with 0 bit output and short source data and transferred buffer during call
Pass	cSHAKE128 with 0 bit output and short source data and transferred buffer after call
Pass	cSHAKE128 with 0 bit output and medium source data
Pass	cSHAKE128 with 0 bit output and medium source data and altered buffer during call
Pass	cSHAKE128 with 0 bit output and medium source data and altered buffer after call
Pass	cSHAKE128 with 0 bit output and medium source data and transferred buffer during call
Pass	cSHAKE128 with 0 bit output and medium source data and transferred buffer after call
Pass	cSHAKE128 with 256 bit output and empty source data
Pass	cSHAKE128 with 256 bit output and short source data
Pass	cSHAKE128 with 256 bit output and short source data and altered buffer during call
Pass	cSHAKE128 with 256 bit output and short source data and altered buffer after call
Pass	cSHAKE128 with 256 bit output and short source data and transferred buffer during call
Pass	cSHAKE128 with 256 bit output and short source data and transferred buffer after call
Pass	cSHAKE128 with 256 bit output and medium source data
Pass	cSHAKE128 with 256 bit output and medium source data and altered buffer during call
Pass	cSHAKE128 with 256 bit output and medium source data and altered buffer after call
Pass	cSHAKE128 with 256 bit output and medium source data and transferred buffer during call
Pass	cSHAKE128 with 256 bit output and medium source data and transferred buffer after call
Pass	cSHAKE128 with 384 bit output and empty source data
Pass	cSHAKE128 with 384 bit output and short source data
Pass	cSHAKE128 with 384 bit output and short source data and altered buffer during call
Pass	cSHAKE128 with 384 bit output and short source data and altered buffer after call
Pass	cSHAKE128 with 384 bit output and short source data and transferred buffer during call
Pass	cSHAKE128 with 384 bit output and short source data and transferred buffer after call
Pass	cSHAKE128 with 384 bit output and medium source data
Pass	cSHAKE128 with 384 bit output and medium source data and altered buffer during call
Pass	cSHAKE128 with 384 bit output and medium source data and altered buffer after call
Pass	cSHAKE128 with 384 bit output and medium source data and transferred buffer during call
Pass	cSHAKE128 with 384 bit output and medium source data and transferred buffer after call
Pass	cSHAKE128 with 512 bit output and empty source data
Pass	cSHAKE128 with 512 bit output and short source data
Pass	cSHAKE128 with 512 bit output and short source data and altered buffer during call
Pass	cSHAKE128 with 512 bit output and short source data and altered buffer after call
Pass	cSHAKE128 with 512 bit output and short source data and transferred buffer during call
Pass	cSHAKE128 with 512 bit output and short source data and transferred buffer after call
Pass	cSHAKE128 with 512 bit output and medium source data
Pass	cSHAKE128 with 512 bit output and medium source data and altered buffer during call
Pass	cSHAKE128 with 512 bit output and medium source data and altered buffer after call
Pass	cSHAKE128 with 512 bit output and medium source data and transferred buffer during call
Pass	cSHAKE128 with 512 bit output and medium source data and transferred buffer after call
Pass	cSHAKE256 with 0 bit output and empty source data
Pass	cSHAKE256 with 0 bit output and short source data
Pass	cSHAKE256 with 0 bit output and short source data and altered buffer during call
Pass	cSHAKE256 with 0 bit output and short source data and altered buffer after call
Pass	cSHAKE256 with 0 bit output and short source data and transferred buffer during call
Pass	cSHAKE256 with 0 bit output and short source data and transferred buffer after call
Pass	cSHAKE256 with 0 bit output and medium source data
Pass	cSHAKE256 with 0 bit output and medium source data and altered buffer during call
Pass	cSHAKE256 with 0 bit output and medium source data and altered buffer after call
Pass	cSHAKE256 with 0 bit output and medium source data and transferred buffer during call
Pass	cSHAKE256 with 0 bit output and medium source data and transferred buffer after call
Pass	cSHAKE256 with 256 bit output and empty source data
Pass	cSHAKE256 with 256 bit output and short source data
Pass	cSHAKE256 with 256 bit output and short source data and altered buffer during call
Pass	cSHAKE256 with 256 bit output and short source data and altered buffer after call
Pass	cSHAKE256 with 256 bit output and short source data and transferred buffer during call
Pass	cSHAKE256 with 256 bit output and short source data and transferred buffer after call
Pass	cSHAKE256 with 256 bit output and medium source data
Pass	cSHAKE256 with 256 bit output and medium source data and altered buffer during call
Pass	cSHAKE256 with 256 bit output and medium source data and altered buffer after call
Pass	cSHAKE256 with 256 bit output and medium source data and transferred buffer during call
Pass	cSHAKE256 with 256 bit output and medium source data and transferred buffer after call
Pass	cSHAKE256 with 384 bit output and empty source data
Pass	cSHAKE256 with 384 bit output and short source data
Pass	cSHAKE256 with 384 bit output and short source data and altered buffer during call
Pass	cSHAKE256 with 384 bit output and short source data and altered buffer after call
Pass	cSHAKE256 with 384 bit output and short source data and transferred buffer during call
Pass	cSHAKE256 with 384 bit output and short source data and transferred buffer after call
Pass	cSHAKE256 with 384 bit output and medium source data
Pass	cSHAKE256 with 384 bit output and medium source data and altered buffer during call
Pass	cSHAKE256 with 384 bit output and medium source data and altered buffer after call
Pass	cSHAKE256 with 384 bit output and medium source data and transferred buffer during call
Pass	cSHAKE256 with 384 bit output and medium source data and transferred buffer after call
Pass	cSHAKE256 with 512 bit output and empty source data
Pass	cSHAKE256 with 512 bit output and short source data
Pass	cSHAKE256 with 512 bit output and short source data and altered buffer during call
Pass	cSHAKE256 with 512 bit output and short source data and altered buffer after call
Pass	cSHAKE256 with 512 bit output and short source data and transferred buffer during call
Pass	cSHAKE256 with 512 bit output and short source data and transferred buffer after call
Pass	cSHAKE256 with 512 bit output and medium source data
Pass	cSHAKE256 with 512 bit output and medium source data and altered buffer during call
Pass	cSHAKE256 with 512 bit output and medium source data and altered buffer after call
Pass	cSHAKE256 with 512 bit output and medium source data and transferred buffer during call
Pass	cSHAKE256 with 512 bit output and medium source data and transferred buffer after call